Rules class #4 tractor pulls

 Tues July 26,2022

 

1. Safety first
2. Always follow the general rules.
3. Maximum 480 cubic inches.
4. Maximum 3”x 3” turbo. No reducers.
5. 20.8 max tire.
6. Roll bar/roll cage and seat belts are MANDATORY!!
7. Intercoolers are allowed, 2.8 turbo LIMIT
8. Water injection is allowed.
9. Any pump up to p7100
10. Driver MUST wear fire suit with gloves and helmet. ALL tractors must be equipped with a Working fire extinguisher.